


   			CA Corner Drive Field Installation

Install the 2-different spacers to the corner drive assembly:  Position corner assembly and spacers as shown below.  Clip each spacer over the corner block on the assembly and then lay it flat to the assembly engaging the spacer tabs into the assembly face.  Add spacers on both sides.
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   Corner Assy & Spacers		Clip spacers onto corner block
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Clip spacers onto corner block          Set spacer flat against Assy
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Corner drive assembly with assembled spacers


Install the corner drive assembly and spacers in the top corner of the main frame and above the tie rod bar.  Ensure the corner drive is flat against the spacers and the spacers are flat against both the jamb and header on both sides.  Attach the assembly with using two screws in each side.
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        Corner Drive Assembly w/Spacers	       2 Spacer (opposite)



Lock the lock assembly (Latch arm down), which positions the tie rod bar to the upper most position.


Push up the bottom of the coupling so the corner drive is fully extended toward the top.
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Set but do not attach the bottom of the tie bar linkage to the vertical tie rod bar top post.
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        		Linkage Bar

Place the linkage against the corner drive coupling and mark where the linkage is below the post above.


Using cutters and plyers, break/trim off the excess linkage length so the linkage will be just below the post above.
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Connect the bottom linkage into the top tie rod bar post and then insert the top of the linkage into the coupling of the corner drive assembly.  May need to punch the linkage bar into the coupling.
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Clip the head tie bar to the corner drive assembly slot on the end of the corner drive.
  [image: ]



On the head tie bar, center the loose spacers between the posts and place the spacer prongs against the interior surface of the header and fasten with screws. 
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Move the latch up and down to verify all connections are good and functioning.


[bookmark: _Hlk121138544]Adding top vertical sash keepers:  The tie rod posts engage the keepers in progression, like a zipper.  Using the lock lever, position the tie rod post for the top existing sash keeper to where it is just at the bottom of the top existing keeper.


Position the top the new top vertical keeper about 1/8” above the top engaging post at the corner drive and anchor the new keeper with the screws.


Keeping the tie rod bar position as identified in steps 12 and 13, position the new head keeper at the same 1/8” distance from the center post on the head tie rod bar and anchor the new keeper with the anchor screws.  The top vertical keeper and the head keeper will engage at the same time.
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Attach horizontal tie bar ta corner drive.
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